(footprint "SW_Push_Wuerth_WS-TASU" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.75 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 03357d91-e1be-4fdf-83f5-dcdb6c6654bd)
  )
  (fp_text value "SW_Push_Wuerth_WS-TASU" (at 0 -4 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5f04213e-c4ff-480a-b2e1-98940ddbadfb)
  )
  (fp_text user "PCB Edge" (at 4.5 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 315d2cc1-6dda-4d1b-9b25-f09153723322)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.75 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9d86fd32-3d61-4d20-a2fe-856bbe2b1ff6)
  )
  (fp_line (start -1.175 2.75) (end 1.175 2.75) (layer "F.SilkS") (width 0.12) (tstamp 1aac8ec5-26f6-4f3a-bae7-aeaa05545820))
  (fp_line (start 1 2.75) (end 1 1.75) (layer "F.SilkS") (width 0.12) (tstamp 3c1fdbf7-27ab-4ade-be3a-bddce2b30b37))
  (fp_line (start -1 2.75) (end -1 1.75) (layer "F.SilkS") (width 0.12) (tstamp 6f74b454-2dcb-4539-a7da-c67b26c07e15))
  (fp_line (start -2.35 1.75) (end 2.35 1.75) (layer "F.SilkS") (width 0.12) (tstamp 755eaeb4-c067-450a-9f8b-0cc64db6b0bd))
  (fp_line (start -2.35 -1.75) (end 2.35 -1.75) (layer "F.SilkS") (width 0.12) (tstamp 7e8c1d22-7db4-482d-8278-a4a315954cbb))
  (fp_line (start -4 -2) (end 4 -2) (layer "F.CrtYd") (width 0.05) (tstamp 3d84fce1-685f-47fe-93ce-0722e082f9c1))
  (fp_line (start 4 -2) (end 4 3) (layer "F.CrtYd") (width 0.05) (tstamp 431fd2bd-cc5f-4abd-ab79-6495011f3668))
  (fp_line (start -4 3) (end -4 -2) (layer "F.CrtYd") (width 0.05) (tstamp ba377ca2-b4cc-4c7c-9c78-43632219214d))
  (fp_line (start 4 3) (end -4 3) (layer "F.CrtYd") (width 0.05) (tstamp eb3df142-f259-4728-a6a0-a3448119a246))
  (fp_line (start 12 2) (end 11 2) (layer "F.Fab") (width 0.1) (tstamp 51f951bf-1c26-4b58-aac2-ef517cdfba31))
  (fp_line (start 7 2) (end 8 2) (layer "F.Fab") (width 0.1) (tstamp 55598805-03cd-432f-a150-86fea1516522))
  (fp_line (start 5 2) (end 6 2) (layer "F.Fab") (width 0.1) (tstamp 76d81342-eb86-4505-ab28-f10f04c8ce1f))
  (fp_line (start 9 2) (end 10 2) (layer "F.Fab") (width 0.1) (tstamp ac0267e1-aa7e-4e5d-82f9-d94c0bb1f165))
  (fp_line (start -4 2) (end 4 2) (layer "F.Fab") (width 0.1) (tstamp cc5d7538-0d93-4314-a7d0-82df8367c71a))
  (pad "1" smd rect (at 2.8 -0.85) (size 1.2 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 35a63c56-361f-42da-9cef-122ce60fabf4))
  (pad "1" smd rect (at -2.8 -0.85) (size 1.2 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 761dcde7-f336-47f6-8855-58bcaea11a91))
  (pad "2" smd rect (at 2.8 0.85) (size 1.2 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d2a1f5d3-8ec8-4476-ac0c-7fee8a4a7bff))
  (pad "2" smd rect (at -2.8 0.85) (size 1.2 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ee869ab0-821c-423e-a344-9a41c14fb260))
)
