(footprint "Inv_F_2.4GHz_TI_AN043" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "modeled after ti an043")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp d9ead5f7-783a-46d9-89f7-f14f2c75eb96)
  )
  (fp_text value "Inv_F_2.4GHz_TI_AN043" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c58d8f4c-0ce3-4005-880f-eaf6a406cecb)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 82887c9d-15ff-4bef-b267-5a447ce02954)
  )
  (fp_text user "Dielectric constant for FR4 is 4.5" (at 12.25 -6.75 unlocked) (layer "User.1")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify right bottom))
    (tstamp 0642c72c-5873-4d33-953b-ccbc57638b1e)
  )
  (fp_text user "PCB DESCRIPTION:1-2 LAYER PCB 0.25 MM NOMINAL" (at 12.25 -10.75 unlocked) (layer "User.1")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify right bottom))
    (tstamp 50c94c5b-a23a-435e-bba3-908f335d62a3)
  )
  (fp_text user "2-3 LAYER PCB 0.50 MM NOMINAL" (at 12.25 -9.75 unlocked) (layer "User.1")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify right bottom))
    (tstamp b7cc7325-73d3-42f5-b366-1be0baade467)
  )
  (fp_text user "THICKNESS FR4 WITH 35um Cu PER LAYER" (at 12.25 -7.75 unlocked) (layer "User.1")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify right bottom))
    (tstamp de0c70fb-12d2-4741-8581-973e1afd2a5d)
  )
  (fp_text user "3-4 LAYER PCB 0.25 MM NOMINAL" (at 12.25 -8.75 unlocked) (layer "User.1")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify right bottom))
    (tstamp f4f29653-d2dc-463b-be94-f4e743a519d3)
  )
  (fp_rect (start -2.55 -5.15) (end 2.45 -4.65)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 8e0d777e-47f5-4611-b993-5410ffe381a2))
  (fp_rect (start -2.55 -4.65) (end -1.65 0.25)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp c731ef91-2dd2-401f-b2c1-7b7fb2bdafb2))
  (fp_rect (start 0.25 0.25) (end -0.25 -4.65)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp ecdbc602-e100-44b7-8b31-0d2f93a15ac8))
  (fp_rect (start 1.95 -4.65) (end 2.45 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 37d0bd6d-6da5-4901-a367-87f516766c69))
  (fp_rect (start 2.45 -2.51) (end 4.45 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 54f1b520-26f3-489b-b141-8b44d8b92659))
  (fp_rect (start 4.45 -5.15) (end 7.15 -4.65)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp ecaac01f-1c98-4262-b4c2-d77c17f7ef5c))
  (fp_rect (start 4.45 -4.65) (end 4.95 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 58832b38-df27-4c4c-a3bf-0f011c56c537))
  (fp_rect (start 6.65 -4.65) (end 7.15 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 56c43f09-1f2b-4ac4-a750-1d1ab817da59))
  (fp_rect (start 7.15 -2.51) (end 9.15 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 421c9b9a-b798-4646-81dc-5a81edd1c4f7))
  (fp_rect (start 9.15 -5.15) (end 11.85 -4.65)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 541d296c-bffe-4017-87cd-37b661c83a38))
  (fp_rect (start 9.15 -4.65) (end 9.65 -2.01)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 73898f0c-2653-4ec2-8dc0-89f3cf75578a))
  (fp_rect (start 11.35 -4.65) (end 11.85 -0.71)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp e1b8f9e7-08d5-44e8-85c7-49beeb4f42cd))
  (fp_rect (start -3.05 -5.45) (end 12.15 0)
    (stroke (width 0) (type solid)) (fill solid) (layer "B.Mask") (tstamp b61dee52-3a69-4bfc-a319-fba70210490c))
  (fp_rect (start -3.05 -5.45) (end 12.15 0)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Mask") (tstamp d5919fc7-9978-408d-80d9-f5a2d56ae310))
  (fp_rect (start -3.05 -5.45) (end 12.15 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp c412b371-f082-484e-afb7-6c0884bb3537))
  (pad "1" smd rect (at 0 0) (size 0.5 0.5) (layers "F.Cu")
    (thermal_bridge_angle 45) (tstamp 540748d7-0b2a-46e1-9fe8-bee508b68f9d))
)
