(footprint "FPC_End_02_P3.00" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e199d134-0cb2-4ce3-a372-9abac689335c)
  )
  (fp_text value "FPC_End_02_P3.00" (at 0 4.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 37ecb86f-2c52-4999-bf2f-40e09b397410)
  )
  (fp_text user "${REFERENCE}" (at 0 6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cd5b54a5-e669-48c4-b8a6-6d2e3abdf655)
  )
  (pad "1" smd rect (at 0 -1.5) (size 3 2.5) (layers "F.Cu" "F.Mask") (tstamp 1569e6b1-eab0-4481-9971-fc7c1faa634d))
  (pad "1" smd rect (at 0 -1.5) (size 3 2.5) (layers "B.Cu" "B.Mask") (tstamp 15dc4d45-85bd-4ba9-bb59-d88d94328520))
  (pad "2" smd rect (at 0 1.5) (size 3 2.5) (layers "F.Cu" "F.Mask") (tstamp e934054a-c808-4a4d-92ee-de1a108bc9ce))
  (pad "2" smd rect (at 0 1.5) (size 3 2.5) (layers "B.Cu" "B.Mask") (tstamp 0e5ace02-296e-40d2-a331-214b07754a89))
)
