(footprint "LED-L1C1_LUMILEDS"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.275391 -2.224609 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "192a245c-c1bf-4009-bc62-156b40062b9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "LED-L1C1_LUMILEDS"
		(at 0.275391 -0.724609 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b0c5f238-cb21-43a9-a5b7-a472fe32ff73")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0.275391 -1.724609 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "18e5e8d8-0056-40e2-b6d5-4881462484a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0.275391 -1.724609 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b034e9d5-e558-4849-b052-fab83a4034f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0.275391 -1.724609 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "66ba7045-9b75-43e3-bd90-b5f346298968")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center 1.5 -0.75)
		(end 1.75 -0.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "664a42ca-af46-46b9-b0bb-ffe28bc2edbc")
	)
	(fp_rect
		(start -1 -1)
		(end 1 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "abbf58b6-03f4-48bf-b1cd-aa03615b9aea")
	)
	(fp_rect
		(start -1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "74d18c48-fcf9-45d1-b734-b313e7bb5370")
	)
	(fp_text user "${REFERENCE}"
		(at 0.275391 0.775391 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f1f42d0d-86fa-4e0a-9d2e-eac9847c9fa4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 0.725 0 270)
		(size 1.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(uuid "882f5294-2b70-41b1-9420-4262530d9012")
	)
	(pad "2" smd roundrect
		(at -0.725 0 270)
		(size 1.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(uuid "bf7397b5-ec79-49a4-9de8-beb7413b4e33")
	)
	(pad "3" smd roundrect
		(at 0 0 270)
		(size 1.7 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "4635f232-4ecc-403b-993d-45336c4c510c")
	)
	(model "$KICAD_USER_3DMODEL_DIR/LUXEON_C_2020_20150108.STEP"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)