(footprint "BarrelJack_Lumberg_161321" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5B191DE1)
  (descr "Barrel jack connector (6mm outer diameter, inner diameter 2.35mm)")
  (tags "connector barrel jack")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.5 0 270) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 73c032d7-ea3b-4237-b31a-fc426f7f7f8b)
  )
  (fp_text value "BarrelJack_Lumberg_161321" (at -15.5 0 270) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4586abf0-479c-42f1-9b2c-2ebfb9cdd513)
  )
  (fp_text user "${REFERENCE}" (at -7.5 0 270) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 547ddf32-ec84-4585-831c-b295f592c871)
  )
  (fp_line (start -13.7 -4.6) (end 1 -4.6) (layer "F.SilkS") (width 0.12) (tstamp 0682d0db-3b86-4fe6-b584-c118d19675d1))
  (fp_line (start -5.2 4.6) (end -13.7 4.6) (layer "F.SilkS") (width 0.12) (tstamp 0dddfe3b-f0be-4942-8102-8468d024e3c3))
  (fp_line (start 1 4.6) (end -0.8 4.6) (layer "F.SilkS") (width 0.12) (tstamp 104be74d-fd49-4464-9292-f479823360a3))
  (fp_line (start 1 -4.6) (end 1 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 2a5ef115-6a9e-49f8-bf6c-db8f63bccf1d))
  (fp_line (start 1.3 -3.2) (end 1.3 -4.9) (layer "F.SilkS") (width 0.12) (tstamp 7ea63b6b-5652-496f-98b9-7ded6e6adac2))
  (fp_line (start 1.3 -4.9) (end -0.3 -4.9) (layer "F.SilkS") (width 0.12) (tstamp 896774bf-a6e6-4512-aeeb-901accd3df1d))
  (fp_line (start -13.7 4.6) (end -13.7 -4.6) (layer "F.SilkS") (width 0.12) (tstamp cde04ee4-6b75-43ae-a314-30f3b1ecacf6))
  (fp_line (start 1 2.5) (end 1 4.6) (layer "F.SilkS") (width 0.12) (tstamp d26ab68a-328c-4bf5-9af9-71a03f060cad))
  (fp_line (start -0.254 5) (end 1.4 5) (layer "F.CrtYd") (width 0.05) (tstamp 04337ed3-ece9-41d4-89c2-79636e098a96))
  (fp_line (start -14.1 5) (end -5.588 5) (layer "F.CrtYd") (width 0.05) (tstamp 4083caf3-83f6-4a86-b2de-9d0453bdd912))
  (fp_line (start -14.1 -5) (end -14.1 5) (layer "F.CrtYd") (width 0.05) (tstamp 4665ad48-c5bb-4ac5-8b09-4bbf273992b5))
  (fp_line (start 1.4 -5) (end -14.1 -5) (layer "F.CrtYd") (width 0.05) (tstamp 53984a07-b2be-42ff-8eab-cf6ceef8cae4))
  (fp_line (start 1.4 5) (end 1.4 -5) (layer "F.CrtYd") (width 0.05) (tstamp 62e0a91a-d976-4402-95a9-9b146ece67df))
  (fp_line (start -0.254 6.604) (end -5.588 6.604) (layer "F.CrtYd") (width 0.05) (tstamp c5f21de7-0b2b-4090-8c56-67f480e63d14))
  (fp_line (start -5.588 6.604) (end -5.588 5) (layer "F.CrtYd") (width 0.05) (tstamp d5ca2006-b256-4ac3-b96b-0b8157b703c9))
  (fp_line (start -0.254 6.604) (end -0.254 5) (layer "F.CrtYd") (width 0.05) (tstamp f7745485-e81f-436d-b53e-4e365c8eff47))
  (fp_line (start -13.6 4.5) (end -13.6 -4.5) (layer "F.Fab") (width 0.1) (tstamp 2efb3af3-df6e-42a5-b44a-d96f7e6c2f83))
  (fp_line (start -13.6 -4.5) (end -0.1 -4.5) (layer "F.Fab") (width 0.1) (tstamp 3cecfda4-f9ef-4d8d-8ad9-96d4f4042102))
  (fp_line (start -0.1 -4.5) (end 0.9 -3.5) (layer "F.Fab") (width 0.1) (tstamp 5b5eaf2a-2415-42bc-89fa-af390ef66b5e))
  (fp_line (start 0.9 4.5) (end 0.9 -3.5) (layer "F.Fab") (width 0.1) (tstamp 64a93e66-27d9-4774-a037-48cbf304c735))
  (fp_line (start 0.9 4.5) (end -13.6 4.5) (layer "F.Fab") (width 0.1) (tstamp a74048fb-b585-4493-8feb-46728cb258e7))
  (pad "1" thru_hole roundrect (at 0 0 270) (size 5 2.5) (drill oval 3.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.5) (tstamp 099bc827-8011-4a85-aabe-4e4e302bdf44))
  (pad "2" thru_hole roundrect (at -6 0 270) (size 4.5 2.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.5) (tstamp d1de6fa5-8f29-4c80-8e50-9a503e5d9a28))
  (pad "3" thru_hole roundrect (at -2.95 4.9) (size 4.5 2.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.5) (tstamp 5d39fec5-4085-460d-88ff-a1f403366a77))
  (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_6941xx301002.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
