(footprint "LED-QLSP07_Quelighting"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.5 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a88a322b-dd2d-4675-a3db-4f75f3396934")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "LED-QLSP07_Quelighting"
		(at 0.5 -1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d2dc8138-e007-4e14-b221-f39c9b865be6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0.5 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bfa82a3e-5d65-4871-b1cb-30e0ed563eef")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0.5 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "52a5a62e-0962-4d9a-a914-b2cbb7ad3316")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0.5 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "070ddb1b-ce21-4a23-a2ad-80818f86af22")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center 2.5 -1.75)
		(end 2.5 -1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "8187d208-e0cd-4b70-9d5f-0206570fb442")
	)
	(fp_rect
		(start -1.75 -1.75)
		(end 1.75 1.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "f383c860-24df-406c-80ae-10c7d83fd12e")
	)
	(fp_rect
		(start -2 -2)
		(end 2 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "4eeed4e4-21a8-4298-9bdf-8b28ae97a086")
	)
	(fp_text user "${REFERENCE}"
		(at 0.5 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e9433f87-7d4e-4b95-96dd-41bf812b3361")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.4 0 270)
		(size 3.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "6d0ebf09-362d-4f3d-90c5-ff91390f43f7")
	)
	(pad "2" smd rect
		(at -1.4 0 270)
		(size 3.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "48104665-ff4b-49d9-bfb3-63b0641abbae")
	)
	(pad "3" smd rect
		(at 0 0 270)
		(size 3.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "417759be-0fad-45c7-8a28-f986251f5c83")
	)
	(model "$KISYS3DMOD/Quelighting_QLSP07 v1.step"
		(offset
			(xyz 0 0 0.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)