(footprint "LED-LV-CRBP.01_OSRAM"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e94eec73-04de-424b-a56a-d95ce0d54f0c")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "LED-LV-CRBP.01_OSRAM"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "298d2ec5-7541-461c-90db-4703a034954b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8b467b57-8b50-458e-9d45-44ca15e40a00")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b26ab521-79c9-430d-854a-f0248c7f2b0a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "60624542-d72e-4777-9c78-bf9573cc8f97")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.3 -1.3)
		(end -0.9 1.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Paste")
		(uuid "145a6eb5-a915-4752-919f-710b1f49fc64")
	)
	(fp_rect
		(start -0.45 -1.3)
		(end 0.45 -0.15)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Paste")
		(uuid "acf3df6f-d43a-4b47-80fe-8c53048c9b90")
	)
	(fp_rect
		(start -0.45 0.15)
		(end 0.45 1.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Paste")
		(uuid "1504b063-e4e8-4360-8f75-ca87415aa048")
	)
	(fp_rect
		(start 0.9 -1.3)
		(end 1.3 1.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Paste")
		(uuid "2596d735-c221-4548-86f1-6cc0b9736c99")
	)
	(fp_circle
		(center 2 1.5)
		(end 2.25 1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "3cdaf358-6274-441b-bb38-b20816fb78fa")
	)
	(fp_rect
		(start -1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "6a29c940-ca78-478a-8c00-ef9a3665ed1d")
	)
	(fp_rect
		(start -2 -2)
		(end 2 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "0030ebfc-f116-4a9b-932b-4d2de945817d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4ada67d7-33d3-4449-b264-3cdc4db83dbe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.125 0 90)
		(size 2.8 0.55)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "28759865-17e6-4ed5-9676-0fe37ebae4a9")
	)
	(pad "2" smd rect
		(at -1.125 0 90)
		(size 2.8 0.55)
		(layers "F.Cu" "F.Mask")
		(uuid "f1b36f0f-30ec-4dba-a974-dec43603a647")
	)
	(pad "3" smd rect
		(at 0 0 90)
		(size 2.8 1)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "99ac4b89-ba73-448c-83ab-2505d6fefbf9")
	)
	(model "$KISYS3DMOD/OSRAM_LV-CRBP.01 v1.step"
		(offset
			(xyz 0 0 0.06)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)