(footprint "BarrelJack_Lumberg_161321"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Barrel jack connector (6mm outer diameter, inner diameter 2.35mm)")
	(tags "connector barrel jack")
	(property "Reference" "REF**"
		(at 2.5 0 -90)
		(layer "F.SilkS")
		(uuid "73c032d7-ea3b-4237-b31a-fc426f7f7f8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "BarrelJack_Lumberg_161321"
		(at -15.5 0 -90)
		(layer "F.Fab")
		(uuid "4586abf0-479c-42f1-9b2c-2ebfb9cdd513")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "05629df1-8ca4-461c-a457-8f3ca21eff18")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6346071f-d002-4903-92c5-d4569171cfe8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a44c8209-bf2b-4086-ba2a-257fad29e0bf")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -13.7 -4.6)
		(end 1 -4.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0682d0db-3b86-4fe6-b584-c118d19675d1")
	)
	(fp_line
		(start -13.7 4.6)
		(end -13.7 -4.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cde04ee4-6b75-43ae-a314-30f3b1ecacf6")
	)
	(fp_line
		(start -5.2 4.6)
		(end -13.7 4.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0dddfe3b-f0be-4942-8102-8468d024e3c3")
	)
	(fp_line
		(start 1 -4.6)
		(end 1 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2a5ef115-6a9e-49f8-bf6c-db8f63bccf1d")
	)
	(fp_line
		(start 1 2.5)
		(end 1 4.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d26ab68a-328c-4bf5-9af9-71a03f060cad")
	)
	(fp_line
		(start 1 4.6)
		(end -0.8 4.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "104be74d-fd49-4464-9292-f479823360a3")
	)
	(fp_line
		(start 1.3 -4.9)
		(end -0.3 -4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "896774bf-a6e6-4512-aeeb-901accd3df1d")
	)
	(fp_line
		(start 1.3 -3.2)
		(end 1.3 -4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7ea63b6b-5652-496f-98b9-7ded6e6adac2")
	)
	(fp_line
		(start -14.1 -5)
		(end -14.1 5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4665ad48-c5bb-4ac5-8b09-4bbf273992b5")
	)
	(fp_line
		(start -14.1 5)
		(end -5.588 5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4083caf3-83f6-4a86-b2de-9d0453bdd912")
	)
	(fp_line
		(start -5.588 6.604)
		(end -5.588 5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d5ca2006-b256-4ac3-b96b-0b8157b703c9")
	)
	(fp_line
		(start -0.254 5)
		(end 1.4 5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "04337ed3-ece9-41d4-89c2-79636e098a96")
	)
	(fp_line
		(start -0.254 6.604)
		(end -5.588 6.604)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c5f21de7-0b2b-4090-8c56-67f480e63d14")
	)
	(fp_line
		(start -0.254 6.604)
		(end -0.254 5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f7745485-e81f-436d-b53e-4e365c8eff47")
	)
	(fp_line
		(start 1.4 -5)
		(end -14.1 -5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "53984a07-b2be-42ff-8eab-cf6ceef8cae4")
	)
	(fp_line
		(start 1.4 5)
		(end 1.4 -5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "62e0a91a-d976-4402-95a9-9b146ece67df")
	)
	(fp_line
		(start -13.6 -4.5)
		(end -0.1 -4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3cecfda4-f9ef-4d8d-8ad9-96d4f4042102")
	)
	(fp_line
		(start -13.6 4.5)
		(end -13.6 -4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2efb3af3-df6e-42a5-b44a-d96f7e6c2f83")
	)
	(fp_line
		(start -0.1 -4.5)
		(end 0.9 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b5eaf2a-2415-42bc-89fa-af390ef66b5e")
	)
	(fp_line
		(start 0.9 4.5)
		(end -13.6 4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a74048fb-b585-4493-8feb-46728cb258e7")
	)
	(fp_line
		(start 0.9 4.5)
		(end 0.9 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "64a93e66-27d9-4774-a037-48cbf304c735")
	)
	(fp_text user "${REFERENCE}"
		(at -7.5 0 -90)
		(layer "F.Fab")
		(uuid "547ddf32-ec84-4585-831c-b295f592c871")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0 270)
		(size 5 2.5)
		(drill oval 3.5 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
		(uuid "099bc827-8011-4a85-aabe-4e4e302bdf44")
	)
	(pad "2" thru_hole roundrect
		(at -6 0 270)
		(size 4.5 2.5)
		(drill oval 3 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
		(uuid "d1de6fa5-8f29-4c80-8e50-9a503e5d9a28")
	)
	(pad "3" thru_hole roundrect
		(at -2.95 4.9)
		(size 4.5 2.5)
		(drill oval 3 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
		(uuid "5d39fec5-4085-460d-88ff-a1f403366a77")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)