(footprint "NetTie_2_0.2mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "NetTie for a 0.2mm trace")
	(property "Reference" "REF**"
		(at 0 -1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "f426310b-ff38-466d-9cd9-8d6001e59086")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "NetTie_2_0.2mm"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "70d3b41f-be4a-4eaf-8b4e-78eb806909c8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0.125 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "47b3d8d5-c488-49b8-9ec4-5b89e460c1aa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0.125 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d41d3056-03fa-45b7-b956-8c13badb4c74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0.125 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1221b5c-7526-493d-bd1e-f71a15023da3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd exclude_from_bom)
	(net_tie_pad_groups "1, 2")
	(fp_rect
		(start -0.25 -0.1)
		(end 0.25 0.1)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Cu")
		(uuid "9217b34d-f3cc-4f9e-8ce6-828b8eb08722")
	)
	(pad "1" smd circle
		(at 0.25 0)
		(size 0.2 0.2)
		(layers "F.Cu")
		(uuid "6c974bbe-2563-4235-a144-9f9c5e5db897")
	)
	(pad "2" smd circle
		(at -0.25 0)
		(size 0.2 0.2)
		(layers "F.Cu")
		(uuid "0122bfbe-1a61-48fa-8f7f-4b3edc578610")
	)
)