(footprint "ST_UFQFPN-20_3x3mm_P0.5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "REF**" (at 0 -3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 698efdaa-d186-408a-a689-757031ac6517)
  )
  (fp_text value "ST_UFQFPN-20_3x3mm_P0.5mm" (at 0 3 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4312fac5-bfd0-478b-88d7-1db8aa79af02)
  )
  (fp_text user "${REFERENCE}" (at 0 -3 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 399a9d74-b944-4177-a01d-49d9629cb896)
  )
  (fp_line (start 1.4 -1.6) (end 1.6 -1.6) (layer "F.SilkS") (width 0.12) (tstamp 273d8fc9-4825-4828-88e2-65aa4c31aede))
  (fp_line (start -1.6 1.6) (end -1.6 1.4) (layer "F.SilkS") (width 0.12) (tstamp 335f7dd6-d43e-4341-bb19-bd9db5e267e6))
  (fp_line (start 1.6 1.4) (end 1.6 1.6) (layer "F.SilkS") (width 0.12) (tstamp 389ef190-7174-4a6b-a91c-3d7ace038944))
  (fp_line (start -1.6 -1.4) (end -1.6 -1.8) (layer "F.SilkS") (width 0.12) (tstamp 69811e26-8cf9-4c1e-9793-cafb5081c494))
  (fp_line (start -1.8 -1.6) (end -1.4 -1.6) (layer "F.SilkS") (width 0.12) (tstamp aa19603a-ed16-4b08-8739-5378fc8d8091))
  (fp_line (start 1.6 -1.6) (end 1.6 -1.4) (layer "F.SilkS") (width 0.12) (tstamp c079bc15-4c38-41a4-891a-f58719e62126))
  (fp_line (start -1.4 1.6) (end -1.6 1.6) (layer "F.SilkS") (width 0.12) (tstamp cf7f6cbd-e590-44ea-8b77-fc162bab5f71))
  (fp_line (start 1.6 1.6) (end 1.4 1.6) (layer "F.SilkS") (width 0.12) (tstamp fae6ebd5-520f-4c13-b9c2-a4793aba4040))
  (fp_line (start 1.9 -1.9) (end 1.9 1.9) (layer "F.CrtYd") (width 0.05) (tstamp 0f240c56-fc17-493d-b79c-d577cb2ea6c5))
  (fp_line (start -1.9 -1.9) (end 1.9 -1.9) (layer "F.CrtYd") (width 0.05) (tstamp 1cda19c5-6c5d-4c27-baee-2ef0637fad3b))
  (fp_line (start 1.9 1.9) (end -1.9 1.9) (layer "F.CrtYd") (width 0.05) (tstamp 991cb7ff-8362-4b24-8bf3-e3aead2eb556))
  (fp_line (start -1.9 1.9) (end -1.9 -1.9) (layer "F.CrtYd") (width 0.05) (tstamp bbeb1de0-ab60-44b8-aa4a-95f069b06832))
  (pad "1" smd custom (at -1.4 -1) (size 0.2 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy -0.25 -0.15)
          (xy 0.1 -0.15)
          (xy 0.25 0)
          (xy 0.25 0.15)
          (xy -0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 9341d3b5-ab28-465a-9f2f-e23942c0d44b))
  (pad "2" smd rect (at -1.3 -0.5 180) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 82504e2a-ec33-46bd-a49e-e7824c6bdcf3))
  (pad "3" smd rect (at -1.3 0 180) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp db58c1d3-9728-4257-879e-d93fa4048a52))
  (pad "4" smd rect (at -1.3 0.5 180) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 84ee3c60-ad3c-4c46-8c45-e2a3ed1c39b1))
  (pad "5" smd custom (at -1.4 1 180) (size 0.2 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0.25 -0.15)
          (xy -0.1 -0.15)
          (xy -0.25 0)
          (xy -0.25 0.15)
          (xy 0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 54f49086-0168-4cee-a425-857e91e0cc27))
  (pad "6" smd custom (at -1 1.4 90) (size 0.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy -0.25 -0.15)
          (xy 0.1 -0.15)
          (xy 0.25 0)
          (xy 0.25 0.15)
          (xy -0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 8b601fee-8af8-4e3f-ae94-1e88be957587))
  (pad "7" smd rect (at -0.5 1.3 270) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp a6946cf1-630a-4fb4-bbb3-7a635f65ffbf))
  (pad "8" smd rect (at 0 1.3 270) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 1c897fe4-1e95-48b5-b82d-1131817a8319))
  (pad "9" smd rect (at 0.5 1.3 270) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 0dcc67fc-cfaa-42dd-960f-f36b4af98a0b))
  (pad "10" smd custom (at 1 1.4 270) (size 0.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0.25 -0.15)
          (xy -0.1 -0.15)
          (xy -0.25 0)
          (xy -0.25 0.15)
          (xy 0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 7431886d-131d-45eb-adb8-0d73242bf952))
  (pad "11" smd custom (at 1.4 1 180) (size 0.2 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy -0.25 -0.15)
          (xy 0.1 -0.15)
          (xy 0.25 0)
          (xy 0.25 0.15)
          (xy -0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp a23bd57a-f715-4604-9342-d02c5dba4dad))
  (pad "12" smd rect (at 1.3 0.5) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp f6acf1a3-7762-4819-b3b9-1676138f1b5b))
  (pad "13" smd rect (at 1.3 0) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp e1b25084-f27a-4b02-861e-59c558c21bd9))
  (pad "14" smd rect (at 1.3 -0.5) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 9cf600c0-2868-42f5-9653-8b857ab1f94b))
  (pad "15" smd custom (at 1.4 -1) (size 0.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0.25 -0.15)
          (xy -0.1 -0.15)
          (xy -0.25 0)
          (xy -0.25 0.15)
          (xy 0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 6c1182e1-15d2-4c42-b541-4e24491750ed))
  (pad "16" smd custom (at 1 -1.4 270) (size 0.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy -0.25 -0.15)
          (xy 0.1 -0.15)
          (xy 0.25 0)
          (xy 0.25 0.15)
          (xy -0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp 5f3ae84f-847c-40f2-865e-fa65c9dca982))
  (pad "17" smd rect (at 0.5 -1.3 90) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp 7bd7497d-6f45-48b2-a050-17eeb12f0c84))
  (pad "18" smd rect (at 0 -1.3 90) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp b93c6155-7cd0-4abb-9609-17a0a3ec6256))
  (pad "19" smd rect (at -0.5 -1.3 90) (size 0.7 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05) (tstamp f3eda014-d483-4c07-b322-541047adb50b))
  (pad "20" smd custom (at -1 -1.4 90) (size 0.3 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.05) (solder_paste_margin_ratio 0.05)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0.25 -0.15)
          (xy -0.1 -0.15)
          (xy -0.25 0)
          (xy -0.25 0.15)
          (xy 0.25 0.15)
        ) (width 0) (fill yes))
    ) (tstamp a727b849-6ade-4763-92d8-5aff71427638))
)
