(footprint "Untitled"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -17.25 -13.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c3477af9-197e-4d08-af5d-e64f292f9b10")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Dealon_XH-4PS"
		(at -17.25 -12 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1b9e6229-d258-4950-bc2a-f075f4e75510")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://jlcpcb.com/api/file/downloadByFileSystemAccessId/8588945156305801216"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "46809410-a1f1-4fea-8ff1-250393a7a37c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "XH 4 Pin Vertical SMD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "72beba7c-d764-479d-8d86-a5838b4b65b7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.81 -3.31)
		(end -4.66 -3.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "995c79b0-1703-4c28-98a1-061b133a8cd7")
	)
	(fp_line
		(start -6.81 -1)
		(end -6.81 -3.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2fab0975-e133-432b-ac1d-35c1d9c9e801")
	)
	(fp_line
		(start -5.79 3)
		(end 5.79 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0c6c66fe-2076-444c-8982-fd60fe1f6993")
	)
	(fp_line
		(start -4.66 -3.31)
		(end -4.66 -6.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec8cff02-aa6a-4b6b-a15b-842ad7141d12")
	)
	(fp_line
		(start 6.81 -3.31)
		(end 4.66 -3.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bc6ebcc8-b644-47b0-be97-db7c190ad8ac")
	)
	(fp_line
		(start 6.81 -1)
		(end 6.81 -3.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "88f21bee-fa79-4b98-bafb-eac122b2faaf")
	)
	(fp_line
		(start -8.35 -7.5)
		(end -8.35 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "03936f3c-4886-4e2a-a19b-9e5feec43132")
	)
	(fp_line
		(start -8.35 4.5)
		(end 8.35 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9640c7a0-6558-4589-be6d-c6524802ddeb")
	)
	(fp_line
		(start 8.35 -7.5)
		(end -8.35 -7.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9c2106d5-b14b-4b71-876c-baf75209ef4a")
	)
	(fp_line
		(start 8.35 4.5)
		(end 8.35 -7.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c08fdaf5-8df6-4794-8131-db60f00085c8")
	)
	(fp_line
		(start -6.7 -3.2)
		(end -6.7 2.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0018655a-c8da-4b27-be59-905eb453d5e9")
	)
	(fp_line
		(start -6.7 -3.2)
		(end 6.7 -3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "821cef1b-1e5b-4545-b699-67d927f6247b")
	)
	(fp_line
		(start -6.7 2.75)
		(end 6.7 2.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "398ae2d9-20a6-4887-b916-cd3926fb801f")
	)
	(fp_line
		(start -4.25 -3.2)
		(end -3.75 -2.492893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5709fbe9-9bfd-4436-b44c-7cb463bdba78")
	)
	(fp_line
		(start -3.75 -2.492893)
		(end -3.25 -3.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0448fcfb-42f6-4db8-85a6-ca744c9b9375")
	)
	(fp_line
		(start 6.7 -3.2)
		(end 6.7 2.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "309490d3-3fc8-4c99-87f0-2b7eee31cc2a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "68631a99-6752-42a5-90be-bb0fecd02c9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.75 -3.25)
		(size 1.3 6.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "0fc9f61a-de83-48a9-9e8c-766eace17143")
	)
	(pad "2" smd roundrect
		(at -1.25 -3.25)
		(size 1.3 6.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "20ed98b4-6cde-4777-9510-647f1f7aad10")
	)
	(pad "3" smd roundrect
		(at 1.25 -3.25)
		(size 1.3 6.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "5e44d1fb-10e1-4cc7-9b40-2bcffb31b9c5")
	)
	(pad "4" smd roundrect
		(at 3.75 -3.2)
		(size 1.3 6.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "a7caca6f-a987-4210-89b5-51fc1dac25f9")
	)
	(pad "MP" smd roundrect
		(at -6.65 0.65)
		(size 1.8 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
		(uuid "7ba783f4-5b33-4019-8bd5-00f22fb3b8a6")
	)
	(pad "MP" smd roundrect
		(at 6.65 0.65)
		(size 1.8 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
		(uuid "a77a06b0-e9dd-4ec6-b394-be17b0c98f78")
	)
	(embedded_fonts no)
)
