(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "4Bit_Level_Shifter_Module" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 3.81 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "4 Bit Level Shifter" (at 3.81 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Seppl_Breakout_Boards:4_Bit_Level_Shifter_Module_Generic" (at 1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 2.794 2.413 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Level-Shifter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "4-Bit Bidirectional Voltage-Level Translator" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Texas*R*PUQFN*N12*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "4Bit_Level_Shifter_Module_0_1"
      (rectangle (start -7.62 6.35) (end 7.62 -6.35)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.54 0)
          (xy -2.54 1.016)
          (xy -0.762 1.016)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.794 0)
          (xy 2.794 -1.016)
          (xy 1.016 -1.016)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 -1.016)
          (xy -2.54 -1.016)
          (xy -2.54 0)
          (xy -4.318 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 -1.016)
          (xy 1.016 0)
          (xy 1.016 -2.032)
          (xy -0.762 -1.016)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 1.016)
          (xy -0.762 0)
          (xy -0.762 2.032)
          (xy 1.016 1.016)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 1.016)
          (xy 2.794 1.016)
          (xy 2.794 0)
          (xy 4.064 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "4Bit_Level_Shifter_Module_1_0"
      (pin bidirectional line (at 10.16 3.81 180) (length 2.54)
        (name "HV1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "4Bit_Level_Shifter_Module_1_1"
      (pin bidirectional line (at -10.16 3.81 0) (length 2.54)
        (name "LV1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 8.89 270) (length 2.54)
        (name "HV" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 1.27 180) (length 2.54)
        (name "HV2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 1.27 0) (length 2.54)
        (name "LV2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 8.89 270) (length 2.54)
        (name "LV" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -8.89 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -1.27 0) (length 2.54)
        (name "LV3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -3.81 0) (length 2.54)
        (name "LV4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -3.81 180) (length 2.54)
        (name "HV4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -1.27 180) (length 2.54)
        (name "HV3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -8.89 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ADS1115_Mod" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -6.35 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ADS1115_Mod" (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ADS1115_Mod_0_0"
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 7.62 180) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 2.54 180) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -2.54 180) (length 2.54)
        (name "ADDR" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -7.62 180) (length 2.54)
        (name "ALRT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ADS1115_Mod_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
    (symbol "ADS1115_Mod_1_1"
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Arduino_Pro_Mini_Variant1" (in_bom yes) (on_board yes)
    (property "Reference" "A" (at 7.62 26.67 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "Arduino_Pro_Mini_Variant1" (at 5.08 -24.13 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "Seppl_Breakout_Boards:Arduino_Pro_Mini_Variant1" (at -12.7 20.32 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at -12.7 22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Arduino pro mini microcontroller module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Arduino Pro Mini Variant 1" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Arduino*Nano*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Arduino_Pro_Mini_Variant1_0_0"
      (pin bidirectional line (at -12.7 20.32 0) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
        (alternate "TX" output line)
      )
      (pin bidirectional line (at -12.7 0 0) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
        (alternate "A_{IN1}" input line)
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "D8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
        (alternate "CLK0" output line)
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
        (name "D9~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -10.16 180) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -7.62 180) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
        (name "D10~" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
        (alternate "SS" output line)
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
        (name "D11~" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
        (alternate "MOSI" output line)
      )
      (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
        (name "D12" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
        (alternate "MISO" input line)
      )
      (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
        (name "D13" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
        (alternate "SCK" output line)
      )
      (pin bidirectional line (at -12.7 17.78 0) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
        (alternate "RX" input line)
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "D14" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
        (alternate "A0" input line)
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "D15" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
        (alternate "A1" input line)
      )
      (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
        (name "D16" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
        (alternate "A2" input line)
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "D17" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
        (alternate "A3" input line)
      )
      (pin power_in line (at 3.81 27.94 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 20.32 180) (length 2.54) hide
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 27.94 270) (length 2.54)
        (name "RAW" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -2.54 180) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 20.32 180) (length 2.54)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
        (alternate "INT0" input line)
      )
      (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
        (name "D3~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
        (alternate "INT1" input line)
      )
      (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
        (alternate "T0" input line)
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "D5~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
        (alternate "T1" input line)
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
        (name "D6~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
        (alternate "A_{IN0}" input line)
      )
    )
    (symbol "Arduino_Pro_Mini_Variant1_0_1"
      (rectangle (start -10.16 25.4) (end 10.16 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
)
