(footprint "LED-XPE2_Cree"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a3f27c0e-67d6-468e-ac8b-76336369ea9f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "LED-XPE2_Cree"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a7da97e7-6295-45f8-929b-5b813cdebe16")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5b971cb9-79a7-47f9-a2b7-243f14f78a6c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c9c7d199-d828-4672-b7c2-2cdb41fb79b1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90038d53-239c-443e-9732-cb87faee294c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center 2.5 1.5)
		(end 2.75 1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "a256e78d-cee2-4915-84e4-c59de9e5c5bb")
	)
	(fp_rect
		(start -1.75 -1.75)
		(end 1.75 1.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Dwgs.User")
		(uuid "31ab98e0-5d07-46ee-aa6b-f399644eafaa")
	)
	(fp_rect
		(start -2.25 -2.25)
		(end 2.25 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "c7580f1e-b832-419b-87bf-b03266440991")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7d11a683-b316-441b-904d-6f365744ae75")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.4 0 270)
		(size 3.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "7202b524-7367-4a7d-be8a-82c15060e997")
	)
	(pad "2" smd rect
		(at -1.4 0 270)
		(size 3.3 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "d086cffd-6ae2-483b-a993-3ee09a495537")
	)
	(pad "3" smd rect
		(at 0 0 270)
		(size 3.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "d35eaf84-0ef4-4688-8572-dbdae23a30f4")
	)
	(model "$KICAD_USER_3DMODEL_DIR/Cree_XPE2 v2.step"
		(offset
			(xyz 0 0 0.05)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)