(footprint "4_Bit_Level_Shifter_Module_Generic" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.160843 0 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 10de62cb-14ae-4a61-b558-47c6d1dc7532)
  )
  (fp_text value "4_Bit_Level_Shifter_Module_Generic" (at 7.62 15.24 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1ac278f1-ae1d-4e89-89c2-f3b155fc1d61)
  )
  (fp_text user "LV | HV" (at 3.81 6.35 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
    (tstamp 9dc66c1a-dd11-47e9-867d-c89b130044fe)
  )
  (fp_text user "${REFERENCE}" (at 6.35 17.78 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 86f52bec-7764-4cde-a8af-8db835273d74)
  )
  (fp_line (start -1.27 -1.27) (end 13.97 -1.27)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 450d6a60-37e0-4c2d-963a-87e73dad049b))
  (fp_line (start -1.27 13.97) (end -1.27 -1.27)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e14ef453-5b2c-429d-9394-f7aed3f99053))
  (fp_line (start 1.27 -1.27) (end 1.27 13.97)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 60dafaac-6be2-45ec-8c70-84ddcdb9b1aa))
  (fp_line (start 1.27 13.97) (end 11.43 13.97)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4ea22fa7-92c1-4524-8fe3-269048640131))
  (fp_line (start 11.43 13.97) (end 11.43 -1.27)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e3e60d24-b308-4747-b705-5618417c5859))
  (fp_line (start 13.97 -1.27) (end 13.97 13.97)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 63189b8f-7589-4bf1-a757-a5d1601767dd))
  (fp_line (start 13.97 13.97) (end -1.27 13.97)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 68ffb081-0ba5-4813-a9d3-a6cff82efcb9))
  (fp_rect (start -1.77 -1.77) (end 1.77 14.47)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 61354198-4560-4f95-be25-af6d6beffe09))
  (fp_rect (start 10.93 -1.77) (end 14.47 14.47)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 25d3ab75-31a2-4997-aea3-d0e6f0237a77))
  (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 0376dbc3-3561-42ac-a328-acb58094de9a))
  (pad "2" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7590b5f6-2a91-4e31-a15d-db9db47d16d0))
  (pad "3" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 758747ae-cbeb-49f9-b42e-22e11a2e25b5))
  (pad "4" thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 46e1be83-55d6-453a-82ab-b6aa65f2d5c7))
  (pad "5" thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ff3282c7-f47c-4537-aba2-74a8a8da971b))
  (pad "6" thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5967c551-1384-4e40-b0e1-f9ca5d7a7563))
  (pad "7" thru_hole circle (at 12.7 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 13f47320-275d-43f7-ad69-e123d9e63f2d))
  (pad "8" thru_hole circle (at 12.7 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2ff404ed-b204-4ef0-8b5f-80371a6b637b))
  (pad "9" thru_hole circle (at 12.7 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2827fb46-1d52-4564-baa2-1de7d5d04bd5))
  (pad "10" thru_hole circle (at 12.7 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 54595a0f-3623-4d3a-86b4-35a31f79ebf3))
  (pad "11" thru_hole circle (at 12.7 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 4635b91b-da67-4277-97bc-f8c4314bbb0f))
  (pad "12" thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 0ec52af2-2f11-4f90-9c43-421d28fa9c8b))
)
