(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Raspberry_Pi_Pico_W_SC0918" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A1" (at 0 58.42 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SC0918" (at 0 55.88 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Raspberry_Pi_Pico_W_SC0918:Raspberry_Pi_Pico_W_SC0918" (at -12.7 -46.99 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf" (at -26.67 -49.53 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "manufacturer" "Raspberry Pi" (at 0 53.34 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "P/N" "SC0918" (at 0 50.8 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "PARTREV" "1.6" (at 0 48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.73mm" (at 0 45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Raspberry Pi Pico W SC0918" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Raspberry_Pi_Pico_W_SC0918_0_0"
      (rectangle (start -20.32 43.18) (end 20.32 -43.18)
        (stroke (width 0.254) (type solid))
        (fill (type background))
      )
      (pin bidirectional line (at -25.4 26.67 0) (length 5.08)
        (name "GP0" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 8.89 0) (length 5.08)
        (name "GP7" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 6.35 0) (length 5.08)
        (name "GP8" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 3.81 0) (length 5.08)
        (name "GP9" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -24.13 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 1.27 0) (length 5.08)
        (name "GP10" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 -1.27 0) (length 5.08)
        (name "GP11" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 -3.81 0) (length 5.08)
        (name "GP12" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 -6.35 0) (length 5.08)
        (name "GP13" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -26.67 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 -8.89 0) (length 5.08)
        (name "GP14" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 24.13 0) (length 5.08)
        (name "GP1" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 -11.43 0) (length 5.08)
        (name "GP15" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 11.43 180) (length 5.08)
        (name "GP16" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 8.89 180) (length 5.08)
        (name "GP17" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -29.21 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 6.35 180) (length 5.08)
        (name "GP18" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 3.81 180) (length 5.08)
        (name "GP19" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 1.27 180) (length 5.08)
        (name "GP20" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -1.27 180) (length 5.08)
        (name "GP21" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -31.75 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -3.81 180) (length 5.08)
        (name "GP22" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -19.05 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -25.4 31.75 0) (length 5.08)
        (name "RUN" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -6.35 180) (length 5.08)
        (name "GP26" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -8.89 180) (length 5.08)
        (name "GP27" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -34.29 0) (length 5.08)
        (name "AGND" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -11.43 180) (length 5.08)
        (name "GP28" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 25.4 26.67 180) (length 5.08)
        (name "ADC_VREF" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 25.4 29.21 180) (length 5.08)
        (name "3V3_OUT" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -25.4 34.29 0) (length 5.08)
        (name "3V3_EN" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -36.83 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin free line (at 25.4 31.75 180) (length 5.08)
        (name "VSYS" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 21.59 0) (length 5.08)
        (name "GP2" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin free line (at 25.4 34.29 180) (length 5.08)
        (name "VBUS" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 19.05 0) (length 5.08)
        (name "GP3" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 16.51 0) (length 5.08)
        (name "GP4" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 13.97 0) (length 5.08)
        (name "GP5" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -25.4 -21.59 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -25.4 11.43 0) (length 5.08)
        (name "GP6" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
