(footprint "Patchfield_08x08"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -15.47 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b762c8e6-a399-4651-93f2-eacac89c226c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Patchfield_08x08"
		(at 0 -13.97 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a2798efa-b005-471d-ae11-e7882898985d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "29a3a298-8f8c-4fdc-9412-a788ad90e79e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Breadboard 08x08"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c4b738dd-7ed0-4c25-887a-e6c2ecabdf53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_bom)
	(fp_rect
		(start -10.16 -10.16)
		(end 10.16 10.16)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "b7486287-d010-476c-a18a-4075eff77df6")
	)
	(fp_rect
		(start -10.16 -10.16)
		(end 10.16 10.16)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "22102966-f8c5-4259-bbeb-f28a578b8902")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -12.47 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6ac5b520-3067-4adf-9356-2da77ee3382b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "A1" thru_hole circle
		(at -8.89 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "027c21c9-dcb3-4eb2-a0d8-25786e4e6253")
	)
	(pad "A2" thru_hole circle
		(at -6.35 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c351c9b5-faa5-4d10-a395-0065cd6ec615")
	)
	(pad "A3" thru_hole circle
		(at -3.81 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5587b88c-2494-46ca-b1cb-7be8ea608066")
	)
	(pad "A4" thru_hole circle
		(at -1.27 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60015c7f-3f65-465f-ba86-968043e6b5d1")
	)
	(pad "A5" thru_hole circle
		(at 1.27 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c413d46-d026-4917-bc6e-d0afaab263c6")
	)
	(pad "A6" thru_hole circle
		(at 3.81 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "00b1ae36-da8a-4629-af73-b78ebfb83883")
	)
	(pad "A7" thru_hole circle
		(at 6.35 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e3782534-073f-45a6-93cc-a81684fceb09")
	)
	(pad "A8" thru_hole circle
		(at 8.89 8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e5868428-ab7a-4931-87f9-6f9fa8e92c71")
	)
	(pad "B1" thru_hole circle
		(at -8.89 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6ba9c23c-a9f1-4cf5-8f45-1b1886cc1aea")
	)
	(pad "B2" thru_hole circle
		(at -6.35 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "75687f20-59b5-4937-a5ba-8cda487e2e5f")
	)
	(pad "B3" thru_hole circle
		(at -3.81 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a5c8c5a0-d2c3-4b6a-8638-bf5dab5a35a2")
	)
	(pad "B4" thru_hole circle
		(at -1.27 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4279a51e-5b5e-4aaf-9305-fbb63aaabb4a")
	)
	(pad "B5" thru_hole circle
		(at 1.27 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ab8d89cc-869a-4f5c-93fb-45af06028bf9")
	)
	(pad "B6" thru_hole circle
		(at 3.81 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ace79bee-473a-4bf2-b4d2-c015dd5f8548")
	)
	(pad "B7" thru_hole circle
		(at 6.35 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f78d8d1-7a80-4909-ace9-d0c78d8ed0e1")
	)
	(pad "B8" thru_hole circle
		(at 8.89 6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0e831216-f289-4fe3-b438-10aa776e822c")
	)
	(pad "C1" thru_hole circle
		(at -8.89 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e01f5d9d-fe97-4351-acf0-1f0a94a07252")
	)
	(pad "C2" thru_hole circle
		(at -6.35 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "93bd20fc-181b-489e-8adc-78ceb87b1efc")
	)
	(pad "C3" thru_hole circle
		(at -3.81 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "aca371f0-24a8-4aa9-8537-efbe8be27e1d")
	)
	(pad "C4" thru_hole circle
		(at -1.27 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3654a357-c555-4beb-93ef-36dd62639f02")
	)
	(pad "C5" thru_hole circle
		(at 1.27 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c925c356-be0b-46b7-827b-cb603ae48bb2")
	)
	(pad "C6" thru_hole circle
		(at 3.81 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8564f6ec-2cc5-4108-89a6-69842614ded4")
	)
	(pad "C7" thru_hole circle
		(at 6.35 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ffb710a8-fcd2-4378-8769-6513913fabfa")
	)
	(pad "C8" thru_hole circle
		(at 8.89 3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6e75d2b3-c39f-4465-ace2-47d462466153")
	)
	(pad "D1" thru_hole circle
		(at -8.89 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "62c17b58-c245-4720-afdc-88c7fbcb58d8")
	)
	(pad "D2" thru_hole circle
		(at -6.35 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a7fc3117-eb83-414e-95f4-eea76a19779a")
	)
	(pad "D3" thru_hole circle
		(at -3.81 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "859b1339-2476-4784-a07d-0e1fd47a04d1")
	)
	(pad "D4" thru_hole circle
		(at -1.27 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c6776f4d-366d-440a-b96a-2366b5b86ac9")
	)
	(pad "D5" thru_hole circle
		(at 1.27 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "717a72ca-f4ff-4b7f-8249-763222e27012")
	)
	(pad "D6" thru_hole circle
		(at 3.81 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fa04299a-af31-4500-ab55-9fd25444c62b")
	)
	(pad "D7" thru_hole circle
		(at 6.35 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e491fcb9-d204-4b0c-993f-cf7d4d31b70f")
	)
	(pad "D8" thru_hole circle
		(at 8.89 1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7159c335-9e49-4fa6-96c7-82ba6a657832")
	)
	(pad "E1" thru_hole circle
		(at -8.89 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "10d9b1d7-d1e6-43fb-aa52-4afb87aeceef")
	)
	(pad "E2" thru_hole circle
		(at -6.35 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2a9f4299-ea2e-4a7d-838c-a0565dd50a67")
	)
	(pad "E3" thru_hole circle
		(at -3.81 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9ed8ac0c-7d4d-4e2e-a45e-31b7a9cb42a5")
	)
	(pad "E4" thru_hole circle
		(at -1.27 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c478d28e-0bf6-4a9c-a7d5-dd6c720b97bc")
	)
	(pad "E5" thru_hole circle
		(at 1.27 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cca60e9a-f9df-424f-ba97-825bc2e2c4e3")
	)
	(pad "E6" thru_hole circle
		(at 3.81 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "febb6aa4-30ec-4b68-aba7-e28700e30183")
	)
	(pad "E7" thru_hole circle
		(at 6.35 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2aa61f51-a68f-459d-a517-aaeb4ba93822")
	)
	(pad "E8" thru_hole circle
		(at 8.89 -1.27 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1945efea-cf1c-426e-a07f-bb2a372be22d")
	)
	(pad "F1" thru_hole circle
		(at -8.89 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "01642fbc-3a5c-4f19-999b-48fbdf581862")
	)
	(pad "F2" thru_hole circle
		(at -6.35 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0d65a210-2160-42ea-9543-1179db852ad4")
	)
	(pad "F3" thru_hole circle
		(at -3.81 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "df0501b3-8162-412f-b497-e9dfcecf050c")
	)
	(pad "F4" thru_hole circle
		(at -1.27 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "73649911-9ace-42e9-b47f-c25c9e166ac4")
	)
	(pad "F5" thru_hole circle
		(at 1.27 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7a5d4784-a012-4da8-adb6-b02913f3c385")
	)
	(pad "F6" thru_hole circle
		(at 3.81 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cd3f28b5-4567-4d8d-a1b1-83af4a5ac430")
	)
	(pad "F7" thru_hole circle
		(at 6.35 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6daec89c-e22d-440b-9ad0-bcdcebcdced6")
	)
	(pad "F8" thru_hole circle
		(at 8.89 -3.81 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "652f0726-6bfb-45d2-b858-a921ff033d4c")
	)
	(pad "G1" thru_hole circle
		(at -8.89 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0041fe98-7457-419e-891d-4a58950a9343")
	)
	(pad "G2" thru_hole circle
		(at -6.35 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "76c037b5-9980-43a3-807b-874a8bb84432")
	)
	(pad "G3" thru_hole circle
		(at -3.81 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ac3b3421-494a-40e6-a600-ff97b76b4a97")
	)
	(pad "G4" thru_hole circle
		(at -1.27 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b2280576-3905-4aa1-9d1c-169f7180e4b7")
	)
	(pad "G5" thru_hole circle
		(at 1.27 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d3dcdd52-ebe8-48ae-a419-5c9d7778f08d")
	)
	(pad "G6" thru_hole circle
		(at 3.81 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "47d360c0-c387-477b-a817-1a475391d293")
	)
	(pad "G7" thru_hole circle
		(at 6.35 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "220ed5fc-1c54-44a4-acae-6c1f4d7311a2")
	)
	(pad "G8" thru_hole circle
		(at 8.89 -6.35 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "358627f2-193e-4058-bc32-3183924246f6")
	)
	(pad "H1" thru_hole circle
		(at -8.89 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "697d61f6-d767-4256-b770-96e17e75c57a")
	)
	(pad "H2" thru_hole circle
		(at -6.35 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "291bf277-dd3c-4496-a833-b77d899e06f9")
	)
	(pad "H3" thru_hole circle
		(at -3.81 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "259aa4f0-c3ef-4994-b6cc-cc5bddb37203")
	)
	(pad "H4" thru_hole circle
		(at -1.27 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "af24e9d5-4fa8-47e6-815a-0fcc774603a9")
	)
	(pad "H5" thru_hole circle
		(at 1.27 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4da584a2-8ed9-4186-ba31-b80f4d353418")
	)
	(pad "H6" thru_hole circle
		(at 3.81 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "faff0e22-a8e0-44d9-b5ab-7cccd46b9662")
	)
	(pad "H7" thru_hole circle
		(at 6.35 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "04b4385c-d33f-41ee-a9ca-ac7c0447b49d")
	)
	(pad "H8" thru_hole circle
		(at 8.89 -8.89 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7df9a866-5343-4426-adc5-5b5a35f16829")
	)
	(embedded_fonts no)
)
